**Arburg Allrounder 370S 800 – 150**

Serial No.: 180

Manufactured: 04/2000

Operating Voltage: 400 v3~ 50Hz

Control Voltage: 230V ~ 50HZ

Control Voltage: 24V

Mot.-Heat.Rated current: 67.0 / 42.0 A

Total rated current: 109.00 A

Total connected load: 64.0 kW

Hydr. Pump operating hours: 53 001 hours

**Including:**

**Suction conveyer VLM 5**

Suction conveyor with integrated collector motor 950W, automatic level monitoring and alarm

signal in case of material shortage. Automatic filter cleaning by compressed air blast. Suitable for granulated and grinded material.

* Stainless steel design
* Wear control of carbon brushes
* Conveying capacity: 50-80 kg/h
* Container volume: 5 liters
* Incl. Material line set 40mm diameter (consising of: intake pipe, hose and 2 hose clamps).

**Compressed air dryer Typ DAC30 N**

Compressed air dryer with molecular sieve

Microprocessor control

Weekly timer

Hopper volume: 30 liters

Air flow:

-6-16 Nm³ / h process

-4 Nm³ / h regeneration

Dew point - 40°C

Heating power 0,95kW

Connected 1kW

Power supply 230V / 50-60HZ

Compressed air connection 6-8bar

Weight 20kg

**FDX-Z color dispenser**

For direct coloring with masterbatch

Fully equipped with:

* Dosing device with control unit for manual setting the dosing time.
* Plexiglass funnel 9ltr
* BA 25 dosing roller