SPECIFICATION SHEET

JAW CRUSHER
MODEL: 30” x 20” RB34 One Piece Frame

HADFIELDS SINGLE TOGGLE ROLLER BEARING JAW CRUSHER

COMPLETE WITH:


Fully Annealed Cast Carbon Steel Main Frame and Jawstock


Plain and Grooved Flywheels


Reversible Manganese Steel Fixed and Swing jaws


Close Fitting Manganese Steel Cheek Plates 

Cartridge Mounted Main Frame Roller Bearings Adequately Sealed by means of Double Labyrinth Seals

Tool Equipment

Operating and Instructions Manual

The specification of the above crusher is as follows:


Size of Feed Opening




: 510 x 762 mm


Minimum Closed Side Setting



: 50 mm


Flywheel Pulley Outside Diameter


: 1349 mm


Eccentric Shaft RPM





: 325 – 350 rpm


Power Required to Drive




: 75 kW


Type of Motor





: 4 Pole


Nett Mass of Crusher




: 10 500 kg


Mass of Main Frame Assembly



: 


Mass of the Swingstock Assembly


: 

THROUGHPUT IN T/H
AT DISCHARGE SETTING OF
WITH 100% PASSING

55
50 mm
75 mm

70
75 mm
130 mm

100
100 mm
150 mm

The above figures are in metric tonnes and are based on crushing limestone weighing about 1 600 kg/m3 (100 lb/ft3) and having a specific gravity of 2.6.  The settings are measured with the jaws in the closed position measured peak-to-valley.  Capacities shown are approximate and will vary with the physical properties of material, moisture content, feed method and feed gradation.

