DGH 555B - Pachette 4

Globally Recognized as the Leading Portable Desktop Pachymeter

**Now Featuring Exclusive Automatic Report Generation Using Bluetooth® Technology.**

[**Click here**](http://www.dghkoi.com/pdf/Pachette4_brochure_full.pdf) **to download the full brochure with Features, Product Specifications, Minimum  
System Requirements and Compatable Operating Systems.**

|  |  |  |  |
| --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | Pachette 4 Ease of Use |  | **EASE OF USE** Turn on power and the Pachette 4 is ready to take measurements. Contact the probe tip to any location on the cornea, and the Pachette 4 will obtain and store up to 25 measurements in less than 2 seconds. Audible feedback indicates when a valid measurement is complete. After bilateral measurements have been completed, the measurements can be reviewed on the 16 character by 2 line LCD which provides easy visibility of the current measurement, the average, and the standard deviation of all measurements taken. | |
|  |
| |  |  |  | | --- | --- | --- | | **ACCURACY & REPRODUCIBILITY** Proven measurement algorithm yields accurate, reproducible measurements in a fraction of a second. The measurement capability of the Pachette 4 is an enhancement of the proven technology that has set the standard for measuring corneal thickness since 1982. |  | Accuracy | |
|  |
| |  |  |  | | --- | --- | --- | | Personolized |  | **PERSONALIZED CONFIGURATION MEMORY** When you receive your Pachette 4, the unit is ready to take corneal measurements at initial power up. It is not necessary to set up or configure any parameters. However, the Pachette 4 has been designed to allow the user to personalize the operational mode, number of measurements taken, adjustment of time delays, etc. Once modified, these parameters are permanently stored in its memory. | |
|  |
| |  |  |  | | --- | --- | --- | | **DURABLE PORTABILITY** The Pachette 4 is designed for performance, portability and convenience, while using limited counter space. The Pachette 4 is encased in a durable rubber holster with a built-in tilt stand. The probe is detachable for easy cleaning and replacement. The probe can be stored in the custom molded probe holder cavity and cord wrap, protecting the probe during transportation or storage. The Pachette 4 has a minimum lifetime of 10 years and an industry leading 3 year warranty. |  | Durable | |
|  |
| |  | | --- | | **ADDITIONAL FEATURES** Mapping Mode for obtaining and storing up to 33 actual and biased corneal mapped measurements. These measurements can be obtained at any point on the cornea, including the periphery.  "Off the shelf" batteries: The Pachette 4 is supplied with 2 sets of NiMh rechargeable batteries (4 total AA batteries). Alkaline batteries can also be used. A battery charger is included with each unit. | |  | |

