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IPS BALERS, INC.


Two Ram Baler Model TR-1388-200
       Revised: 6/06
HYDRAULIC


Main Pumps
596 GPM Total Flow (Regen. System) 


System Pressure
3200 PSI


Main Cylinder
13 In Bore


Ejector Cylinder
9 In Bore


Bale Door Cylinder
8 In Bore


Precompression Cyl.
8 In Bore (Optional)


Total Force
424,530 Lb


Ram Face Pressure
253 PSI


Oil Reservoir
1500 Gallon Capacity 



L&P Wire-Tie or Accent Wire- Tire
ELECTRICAL


Main Motor
Two (2) 100 HP, 460 Volt, 3 Phase, TEFC, Special Duty, Wye Delta Starting


Cooler Pump Motor
7.5 HP, 460 Volt, 3 Phase


Cooler Fan Motor
Two (2) 3 HP, 460 Volt, 3 Phase


Strapper Pump Motor
10 HP, 460 Volt, 3 Phase


Controls  
Programmable Controller with Diagnostics and Phone Modem


Photocell
Infrared Type

STRUCTURAL 


Length Overall
36 Ft 


Hopper Opening
96 In Long x 72 In Wide (W/Lid 90 In Long x 60 In Wide)


Charge Box Opening
96 In Long X 57.5 In Wide (W/Lid 90 In Long x 57.5 In Wide)


Width Overall
21 Ft 0 In


Charging Hopper Ht.
7 Ft 6 In (With Lid 13 Ft 1 In)


Shear Blade
Knife Steel, Reversible


Liners
Hardox 400 or Equal  (Charging Box totally lined w/wear plates)


Shipping Weight
53 Tons Approximate (With Lid 57 Tons)

PERFORMANCE


Bale Size
45 In Wide x 30 In High x 62-64 In Length


Bale Volume 
50 Cubic Feet Expanded (Approximate)


Cycle Time
9 Seconds (No Load – Main Cylinder Only)


Bale Time
72 Seconds (Strapper Time Included)



*(3 Strokes/Bale) Estimated for OCC W/Lid

	Material
	Material PCF

Infeed Density
	Bale Weight

LB
	Density  PCF

Baled
	Output 

No Lid

Tons per Hr
	Output 

With Lid

Tons per Hr

	*OCC
	2.5 -  4
	up to 1500
	up to 30
	up to 24
	up  to 24

	*News
	6 - 8
	up to 1700
	up to 34
	up to 40
	up to 40

	*PET
	.75 - 4
	up to 1250
	up to 25
	up to 9
	up to 10

	*UBC
	1.5 - 4
	up to 1200
	up to 24
	up to 16
	up to 18

	*Solid Waste
	8 - 12
	up to 2500
	up to 50
	up to 44
	up to 46

	*Carpet Waste
	2.5 -  4
	Up to 1500
	Up to 30
	Up to 18
	up to 18


*Performance Rates, Bale Weights, and Bale Densities Are Subject to Moisture Content, Material Pre-Bale Densities, 

Feed Rates, And Other Variables in Baling

STANDARD FEATURES




AVAILABLE OPTIONS
Programmable Controller with Phone Modem

Pre Compression Lid

Oil Cooler and Oil Heater 



Conveyor Controls

Bale Door / Relief 



Feed Hopper Extension with Upper Level Sensor

Wye-Delta Starting 



Contact Factory for other Options

Hydraulic Pumps Submerged in Oil to Eliminate Cavitation

Specifications and Design are Subject to Change if, in the opinion of the Manufacturer, the Change is an improvement.
P. O. Box 414

800-280-2313

396 Frost Industrial Boulevard

912-366-9460

Baxley, GA 31513

Fax 912-366-9559


