MODELS DHW DHWS
HEAVY DIJTY DOWNSTROKE BALING PRESS
Sulidl'/ constructed 01 quality materials b'/ expert craftsmen, this press boosts Ill the extra features thot howe estohF15hed Consolidated as the worldwide leader in the Inunufoctwre of superior hydrauli( buling presses, Il','fillnhle in Single double chornber models Recommended for the duty bcling of wiping mgs, Clothing, textile towels, etc,D*WS-SINGLE

Features:
· Retructuble End Doors-permit complete wmpping of the bole while ill the 	5inre all four sides of bole 	exposed.
· Simpfified Controls-simple ditecticnol With pushbutton operation.
	
	
	WASTE TECHNOLOGY CORPORATION[image: ]

	
	
	


[image: ]•Self Contained Unit-motor, pump, outumotic IBIief oll controls cre ntttthed to press—no pil 01 specinl foundation [equired.
· [image: ]UL Listed Panel-ensures the electlitfil panel meets today's quoliT,' stnnd01ds.
· Moveable Retainer Dogs (optional)-f01 Ille baling of fluff} motericls where multiple Imdngs and ctmpÆ5iijns are necessity.
DOUBLE CHAMBER DOWNSTROKE BALING PRESS Additional Features:
· Double Chamber-one chnrnbgr is IOCldgd while bole ill tie opposite (homher is compressed, 'Overed and lied. After removing the finished bole. the Chomhers ore revolved and the filled chomber is howght in position for compression. This [image: ]operation saves time and[image: ]
· Loading Options-permit loading of the [image: ]the some [image: ]the floc)' both.
DHW-DOUBLE CHAMBER
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Double Chambes Medel - Chamber Size Dimensions {inches & mm) Shipping Wt. Singee Chamber Mool Chamber Size limenstons [nches & many Sfippng W

OHW-1 inches 1601648 B4 30 1 2,600 lbs. DHWS-1 inches 16x30x48 60 30 M9% 2,200 ks

DEW-1 mm 06l 19 N 162 3097 1,179 ka. DHWS-1 mm 406762219 1537 762 3035 798 ko
D2 inches T6xa0xdd 12 30 126 3,650 |bs. DHWS-2 inches 3654 6% 30 126 2850Ms
DHW-2* mm 4067620219 7845 762 3200 1856 ky. DHWS2 o S0BN372 1943 76T 30 1193k
OHW-3C inches 16x30x60 12 30 153 4,675 [bs. DHWS:3 inches Ddyd2xb0 Te 40 138% 4,400 ks,
DHW-3Cmm 4067621524 2845 762 3886 2121 by DHWS3 mm  610¢1067x1524 2146 1016 3467 2087 kg
DHW-3CHD inches 163060 nl 40 157 6,400 lbs. DHWS inches  DdxdBub0 845 40 140 5,300 Ibs.
DHW3CHD mm  406a762a1524 2845 1016 3988 2903 kg. DHWS-4 mm G10:762a1524 2146 1016 3556 HDd kg
DHW-4 inches 20x36x54 1M kL 138 4,700 lbs. DHWSS inches Ddxdbi? 85 45 154% 6,300 bs.
DHW-4 mm 508:91441372 3150 B4 3505 2132 by, DHWS-5 mm S10hTE2082% 177 1143 3918 2658 kg
DHWS inches Hedlatl) 148 36 154 7,500 lbs. DHWS-6 inches y54a w% 47 17 7000 ks
DHW-5 mm 610:1067x1524 3759 4 392 34072 kg. DHWS6mm 686137261981 2350 1194 4496 3175 kg
DHW-G inches Tudxtl 156 40 160 8,500 Ibs. DHWS inches I0x60x78 96% 50 180 7,800 lbs.
DHW-6 mm 61047621524 3962 1016 4064 3856 kg. DHWS mm 76215241961 2502 1270 4572 3538 kg

DHW-7 inches Hxdlar2 156 47 178 9,400 1bs.
DHW-7 mm S10:762x16829 3962 1069 4521 4264 kg,
DHW-G inchas 5478 174 12 190 10,5000
DHW- mm 6861371981 4420 1069 4826 4763 kg
DHW-? inches J0x60x78 186 4 196 11,500 fbs.
DHW-3 mm ThIx1SMx1981 4724 1069 4978 5216 kg,
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