SPECS OF UNIT
Manufacturer: Production Facilities Equipment Co., Inc.
Serial #: VS-3018-0118
 This unit is a:
Truck-Mounted LACT Separator (Skid Unit)
From auction/field data, that exact serial number corresponds to:
· 18" OD vessel 
· Approx 4 ft x 15 ft separator body 
· Skid-mounted package 
· Designed for LACT (Lease Automatic Custody Transfer) service 
Separator Vessel
· Oil/water separation before measurement 
· Non-code vessel (common for field units) 
Pump System
· Gorman-Rupp gear pump 
· ~3 HP motor (Class I Div 2 rated) 
· 2.5" NPT connections 
· Built-in relief (30–95 PSI range) 
Skid
· Open oilfield skid 
· Roughly 7.5' x 6.5' footprint 
 What It’s Used For
This is standard in:
· LACT units (custody transfer) 
· Tank batteries 
· Truck loading/unloading 
· Oilfield production sites 
Basically:
Separates fluid → pumps it → sends it through meter for sales

Rosemount 3051CD Differential Pressure Transmitter
3051CD = Coplanar Differential Pressure Transmitter
 Accuracy: up to ±0.075% of span 
Output: 4–20 mA + HART 
Pressure capability: varies by range (often up to 2,000+ psi line pressure) 

Long-term stability: designed for 15+ years service
Tornado Meter (Calgary, Alberta, Canada)
· Positive displacement / inline flow meter or flow element 
· Used in LACT measurement systems
Measures fluid volume very accurately before custody transfer 

Pump Package
· Gorman-Rupp gear pump 
· Electric motor driven ( ~3 HP) 
· Moves product through the meter

