OILWELL E 2000HP

OILWELL E-2000 single drum draw works with Elmagco 7838 electric brake and (2) GE 752’s

LEE C MOORE cantilever mast 142’ x 1,300,000 lbs SHL, 9 sheave crown grooved for 1 1/2” wire line

LEE C MOORE swing-up substructure, 30’ floor height, 26’ clear height, 1,000,000# rotary capacity with 800,000 # setback capacity

(2) OILWELL A-1700 PT triplex mud pump, rigged out with (2) GE 752’s

ROSS HILL model 1400, 4 bay SCR (rebuilt)

CANRIG 500 ton top drive with drive house

NATIONAL IR 3080 Iron rough neck

OILWELL 500 ton block with BJ 5500 Dynaplex hook

NATIONAL P-650 swivel

OILWELL 27 1/2” rotary table

KOOMEY 180 gal 7 station air and electric accumulator with remote

CHOKE MANIFOLD

(3) CATERPILLAR D399TA’s each with KATO 1050 KW generators, cold start and wired

(3) Mud tanks with stirrers, shakers, electric centrifugal pumps, de sander, de slilter, cyclone

10’ x 45’ pusher house

air compressors, trip tank, Oil bin, catwalk, driller dog house, ODS dog house, mixing house, fuel tank, derrick stand, water tanks, suitcases, survey unit, storage house and many extra’s