**ERFURT BILLET SHEAR 500 TON**

* Cold cut capacity: 500 TON
* Stroke per minute: 25
* Knife lenght: 420 mm
* Stroke sledge hammer: 100 mm
* Power: 1 motor AC 37 kW
* Weight: about 20 TON
* Condition: second hand completely revamped

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Cold cut capacity with R - kg/mm2** | | | **45** | **50** | **60** | **70** | **80** | **90** |
|  | **Square section billets side, in mm** | **Without holder** | 125 | 118 | 106 | 95 | 85 | 75 |
| **With holder** | 115 | 108 | 95 | 85 | 75 | 70 |
|  | **Round section billets diameter, in mm** | **Without holder** | 132 | 125 | 112 | 100 | 90 | 80 |
| **With holder** | 120 | 115 | 100 | 90 | 80 | 75 |
|  | **Rectangular profil in mm** | | 375X50 | 375X45 | 375X40 | 375X35 | 375X32 | 375X28 |
|  | **Rectangular profil in mm** | | 280 X60 | 280X55 | 280X45 | 280X40 | 280X35 | 280X30 |